PAN ID: ABC  
Channel: C

Manager MY: 0x01  
  
Controller Triangle Red MY: 0x39  
Controller Triangle Blue MY: 0x3A  
Controller Triangle Green MY: 0x3B  
Controller Triangle Yellow MY: 0x3C  
Controller Triangle Purple MY: 0x3D  
Controller Triangle Black MY: 0x3E  
Controller Triangle Orange MY: 0x3F

Scoreboard MY: 0x05

Triangle 0x0-  
Square 0x1-  
Circle 0x2-

//don’t need API mode on derby nodes, it just prints the payload…

|  |  |  |
| --- | --- | --- |
| License Shape | License Color | MY Address |
| Triangle | Red | 0x09 |
| Triangle | Blue | 0X0A |
| Triangle | Green | 0x0B |
| Triangle | Yellow | 0x0C |
| Triangle | Purple | 0X0D |
| Triangle | Black | 0X0E |
| Triangle | Orange | 0x0F |
| Square | Red | 0x19 |
| Square | Blue | 0X1A |
| Square | Green | 0x1B |
| Square | Yellow | 0x1C |
| Square | Purple | 0X1D |
| Square | Black | 0X1E |
| Square | Orange | 0x1F |
| Circle | Red | 0x29 |
| Circle | Blue | 0X2A |
| Circle | Green | 0x2B |
| Circle | Yellow | 0x2C |
| Circle | Purple | 0X2D |
| Circle | Black | 0X2E |
| Circle | Orange | 0x2F |

|  |  |
| --- | --- |
| Router Name | MY Address |
| Manager | 0x01 |
| Router 1 | 0x02 |